{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Acél","Keményfém"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Acél","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,2,1,6],[2,2,2,6]]}
[]
["BMEattNyP",null,"ACÉL ELŐFESZÍTETT SZERSZÁM MÉRETEZÉSE"]
[null,null,"Osman-Zombori: Hidegalakítószerszámok méretezése"]
[]
[null,"SZÁMOL"]
[]
[]
[null,"Rk:",52.695915440688871,null,"amin:",2.6347957720344435,null,"p1max:",900]
[]
[null,"n","ki","Ei","mi","ai","Rbi","di"]
[null,null,1500,210000,0.3,1.6514456476895409,20]
[null,null,1400,210000,0.3,1.5954480704349314,33.028912953790822,0.13368845719391531]
[null,null,null,210000,0.3]
[null,null,null,210000,0.3]
[null,null,null,210000,0.3]
[]
[null,"p2`:",190.92489568845627,null,"stb:",602.92072322670401,null,"pkrit:",6229.2486169134118]

{"sheet":"Keményfém","index":1,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,2,1,7],[2,2,2,7]]}
[]
["BMEattNyP",null,"KEMÉNYFÉM-ACÉL ELŐFESZÍTETT SZERSZÁM MÉRETEZÉSE"]
[null,null,"Osman-Zombori: Hidegalakítószerszámok méretezése"]
[]
[null,"SZÁMOL"]
[]
[]
[null,"Rk:",123.25166214790868,null,"amin:",4.9300664859163472,null,"p1max:",1500]
[]
[null,"n","ki","Ei","mi","ai","Rbi","di"]
[null,null,50000,500000,0.25,1.5811388300841898,25]
[null,null,1500,210000,0.3,1.5811388300841898,39.528470752104745,0.15881974855756356]
[null,null,1400,210000,0.3,1.527525231651947,62.500000000000007,0.23809523809523817]
[null,null,1000,210000,0.3,1.2909944487358056,95.470326978246703,0.18184824186332726]
[null,null,null,210000,0.3]
[]
[null,"p2`:",700.62586926286508,null,"stb:",2335.4195642095501,null,"pkrit:",11413.151741708516]